**14148 – USB Temperature Only Data Logger**

Dimensions 99 x 25 x 23mm

Use the USB Temperature Only Data Logger to measure, store and track over 16,000 readings in a -35°C to +80°C temperature range. Set alarm thresholds and choose how often you would like temperatures to be logged from every 10 seconds to 12 hours and when you want it to start logging data with the option of immediate or delayed start.

See the data from the temperature logger by downloading the free EasyLog Software where it will load the results into graphs that can be exported to other applications for analysis. The software runs under Windows® 7, Windows® 98/2000/XP (Home and Professional Editions) Vista® (32-bit only).

The data logger uses two LEDs that can flash in combinations of red, amber and green to show its status such as when it has completed logging data. The LED lights also have an indicator for if an alarm level has been exceeded.

The data logger is supplied with one 1.5V alkaline battery with a life of 3 years and is protected against moisture to IP67 standard when the protective cap is fitted securely on the device.